//*******************************************************//
//  TELESIS TELEKOMUNIKASYON SISTEMLERI SAN VE TIC A.S.  //
//                                                       //
//            PX24N (Telesis Nano) IP PBX                //
//             Easy Installation Utility                 //
//                                                       //
//              Release Date: 2011.03.30                 //
//                   Version: v1.2dr                     //
//*******************************************************//

Thank you for purchasing the PX24N (Telesis Nano) IP PBX system


------------------------CONTENTS----------------------------

1) PX24N Features
2) PC Requirements
3) Starting the Installation
4) Troubleshooting
5) Contacts

-----------------------------------------------------------

1) PX24N Features:

Each PX24N comes with the following standard hardware and software features

    * 3 analog DC loop trunks (i.e., CO trunks or FXO ports)
    * 3 analog subscribers (FXS ports)
    * Caller ID encoders (transmitters) for all FXS ports
    * Caller ID decoders (receivers) for all FXO ports
    * 10 SIP, or H.323, or xSIP local users or trunks
    * 3 concurrent VoIP-TDM calls (gateway channels)
    * Hosted Java WebPhone client applet
    * DTMF transceivers
    * Conference hardware
    * Integrated CMDR (call records) buffer
    * Integrated DVR (digital voice recorder) with 100 hours (6000 minutes) capacity
    * 4 playing and 4 recording channels for the DVR
    * Personal conversation recording capability
    * Integrated Voice Mail (VMail)
    * Integrated Automatic Call Distributor
    * Integrated Web server
    * Integrated API server
    * Data link for adjunct call processing servers
    * XDP (Xymphony Discovery Protocol) support
    * Mains power adapter 
    * Hundreds of supplementary services for analog, digital and VoIP users
    * Integrated feature phone with the following capabilities and features 
          o backlighted, graphic LCD with 8 rows, 25 columns
          o 62 keys in total
          o 4x3 keypad, continuously backlighted for fashion and usability
          o navigation keys
          o call park keys
          o call record key
          o call transfer key
          o volume control keys 
          o shift function key
          o 30 quick access keys (120 quick access with using the Shift key)
          o redial key
          o transfer key
          o disconnect key
          o conference key
          o speakerphone key
          o mute key
          o flash key
          o function keys
          o text keypad 
          o headphone jack
          o microphone jack
          o missed calls listing
          o dialed numbers listing
          o incoming calls listing
          o phone directory
          o playing, deleting voice messages and recorded conversations
          o ringer melody selection
          o setting call forward unconditional
          o setting call forward busy
          o setting call forward no-reply
          o setting hotline
          o activating call waiting
          o activating do not disturb
          o activating wake-up (reminder) service
          o deflecting calls
          o activating call back
          o holding calls on
          o retrieving calls
          o transferring calls
          o tracing transferred calls (up to 4 calls)
          o activating conference
          o recording the conversation bi-directionally (both calling and called 
          party voices)

-----------------------------------------------------------

2) PC Requirements:

Windows XP SP2 / Vista / Seven	
1.00GHz or better processor
Minimu 512mb RAM
Minimum 100MB free disk space
Voice card
Ethernet
CD driver	
Java Runtime Environment (JRE) Version 6 Update 19  (*) 
Microsoft C++ Redestributable Package (**)	 

(*) If JRE has not been installed in your PC, this Easy Installation utility does
not start. Then you may install JRE, which is available in JAVA directory of this
CD. 

(**) If Microsoft C++ Redestributable Package has not been installed in your PC,
this Easy Installation utility asks you to install it. Please allow the installation.
Be aware that Xcom, Xphone and XTools programs will not run unless Microsoft C++ 
Redestributable Package has been installed.

-----------------------------------------------------------

3) Starting the Installation

Install the CD into the CD driver of your PC. If Easy Installation utility does
not start automatically then you may manually run Setup.exe in the CD. To remind
you, if your PC asks confirmation to run the utility, you must allow it.

Be aware that your PC shall meet the requirements mentioned above.

At the beginning, select your language for the installation. Then click on the 
“Intallation” button. In the pulldown menu, select the system model as "PX24n"
and  click on the “Intall” button to start the installation. Follow all the steps
in proceeding pages to complete your installation.

-----------------------------------------------------------

4) Troubleshooting

CD does not start up!
Run Setup.exe in the CD manually. To remind you, if your PC asks confirmation to 
run the utility, you must allow it.

Setup.exe does not run!
There may be a physical damage on the CD. Download the CD image from our web site.

PX24N does not start up!
Be sure if the PX24N is powered up

XTools, XCom, or XPhone programs do not start up!
Be sure that you have allowed the installation of Microsoft C++ Redestributable 
Package. If not, re-try the installation and allow the package to be installed.

Install Java Runtime error appears!
Run jre-6u18.exe, which is available in JAVA directory of the CD. Then re-try the
installation.

-----------------------------------------------------------

5) Contacts

For any of your problems, we advice you to contact your reseller first.

Besides you may also check documentation available at:

http://www.telesis-pbx.com 

Thank you.

--END--


























